(export (version D)
  (design
    (source C:\Users\Kevin\Documents\Projects\NixieTubeClock\Nixie_Top_Board\nixie_top_board.sch)
    (date "7/30/2018 8:46:50 PM")
    (tool "Eeschema (5.0.0)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Top Board")
        (company "Nixie Tube Clock")
        (rev A)
        (date 2017-06-08)
        (source nixie_top_board.sch)
        (comment (number 1) (value https://0x7d.com/2017/nixie-tube-clock/))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref T3)
      (value IN-8)
      (footprint "Custom Parts:IN-8")
      (libsource (lib Custom_Parts) (part IN-8) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FA0F))
    (comp (ref T2)
      (value IN-8)
      (footprint "Custom Parts:IN-8")
      (libsource (lib Custom_Parts) (part IN-8) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FA7E))
    (comp (ref T1)
      (value IN-8)
      (footprint "Custom Parts:IN-8")
      (libsource (lib Custom_Parts) (part IN-8) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FAE9))
    (comp (ref T4)
      (value IN-8)
      (footprint "Custom Parts:IN-8")
      (libsource (lib Custom_Parts) (part IN-8) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FB49))
    (comp (ref Q31)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FCEB))
    (comp (ref Q32)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FF4E))
    (comp (ref Q33)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5938FF9A))
    (comp (ref Q34)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939000A))
    (comp (ref Q35)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59390080))
    (comp (ref Q36)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593905DE))
    (comp (ref Q37)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593905E4))
    (comp (ref Q38)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593905EA))
    (comp (ref Q39)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593905F0))
    (comp (ref Q40)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593905F6))
    (comp (ref Q21)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939343C))
    (comp (ref Q22)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393442))
    (comp (ref Q23)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393448))
    (comp (ref Q24)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939344E))
    (comp (ref Q25)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393454))
    (comp (ref Q26)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939345A))
    (comp (ref Q27)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393460))
    (comp (ref Q28)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393466))
    (comp (ref Q29)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939346C))
    (comp (ref Q30)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393472))
    (comp (ref Q11)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936AA))
    (comp (ref Q12)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936B0))
    (comp (ref Q13)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936B6))
    (comp (ref Q14)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936BC))
    (comp (ref Q15)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936C2))
    (comp (ref Q16)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936C8))
    (comp (ref Q17)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936CE))
    (comp (ref Q18)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936D4))
    (comp (ref Q19)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936DA))
    (comp (ref Q20)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936E0))
    (comp (ref Q1)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936E6))
    (comp (ref Q2)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936EC))
    (comp (ref Q3)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936F2))
    (comp (ref Q4)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936F8))
    (comp (ref Q5)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593936FE))
    (comp (ref Q6)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393704))
    (comp (ref Q7)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939370A))
    (comp (ref Q8)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393710))
    (comp (ref Q9)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 59393716))
    (comp (ref Q10)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5939371C))
    (comp (ref U1)
      (value PCA9685)
      (footprint Housings_DFN_QFN:QFN-28-1EP_6x6mm_Pitch0.65mm)
      (libsource (lib Custom_Parts) (part PCA9685) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 593A4DD3))
    (comp (ref U2)
      (value PCA9685)
      (footprint Housings_DFN_QFN:QFN-28-1EP_6x6mm_Pitch0.65mm)
      (libsource (lib Custom_Parts) (part PCA9685) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 593A4ED6))
    (comp (ref U3)
      (value PCA9685)
      (footprint Housings_DFN_QFN:QFN-28-1EP_6x6mm_Pitch0.65mm)
      (libsource (lib Custom_Parts) (part PCA9685) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 593A4FC1))
    (comp (ref Q41)
      (value Q_NPN_BEC)
      (footprint TO_SOT_Packages_SMD:SOT-323_SC-70)
      (libsource (lib Device) (part Q_NPN_BEC) (description "Transistor NPN (general)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 593B48A7))
    (comp (ref T5)
      (value IN-3)
      (footprint "Custom Parts:Phoenix_1770953")
      (libsource (lib Custom_Parts) (part IN-3) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 593B460C))
    (comp (ref R1)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D252E))
    (comp (ref R2)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D296E))
    (comp (ref R3)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2A32))
    (comp (ref R4)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2AF9))
    (comp (ref R5)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2BC7))
    (comp (ref R6)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2CD3))
    (comp (ref R7)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2DA3))
    (comp (ref R8)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2E76))
    (comp (ref R9)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D2F4C))
    (comp (ref R10)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3025))
    (comp (ref R11)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3315))
    (comp (ref R12)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D331B))
    (comp (ref R13)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3321))
    (comp (ref R14)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3327))
    (comp (ref R15)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D332D))
    (comp (ref R16)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3333))
    (comp (ref R17)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3339))
    (comp (ref R18)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D333F))
    (comp (ref R19)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3345))
    (comp (ref R20)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D334B))
    (comp (ref R21)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3543))
    (comp (ref R22)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3549))
    (comp (ref R23)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D354F))
    (comp (ref R24)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3555))
    (comp (ref R25)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D355B))
    (comp (ref R26)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3561))
    (comp (ref R27)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3567))
    (comp (ref R28)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D356D))
    (comp (ref R29)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3573))
    (comp (ref R30)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3579))
    (comp (ref R31)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3771))
    (comp (ref R32)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3777))
    (comp (ref R33)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D377D))
    (comp (ref R34)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3783))
    (comp (ref R35)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3789))
    (comp (ref R36)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D378F))
    (comp (ref R37)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D3795))
    (comp (ref R38)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D379B))
    (comp (ref R39)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D37A1))
    (comp (ref R40)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593D37A7))
    (comp (ref C1)
      (value Bypass)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948AC88))
    (comp (ref C2)
      (value Bypass)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948AFF9))
    (comp (ref C3)
      (value Bypass)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5948B9CD))
    (comp (ref R41)
      (value R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 593DC6D8))
    (comp (ref J1)
      (value Conn_02x03_Odd_Even)
      (footprint "Custom Parts:Pin_Header_Straight_2x03_Pitch2.00mm")
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x03_Odd_Even) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B59228D))
    (comp (ref J2)
      (value Conn_02x03_Odd_Even)
      (footprint "Custom Parts:Pin_Header_Straight_2x03_Pitch2.00mm")
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x03_Odd_Even) (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B592538)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_02x03_Odd_Even)
      (description "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x03_Odd_Even))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Custom_Parts) (part IN-3)
      (fields
        (field (name Reference) T)
        (field (name Value) IN-3))
      (pins
        (pin (num 1) (name A) (type input))
        (pin (num 2) (name C) (type input))))
    (libpart (lib Custom_Parts) (part IN-8)
      (fields
        (field (name Reference) T)
        (field (name Value) IN-8))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))
        (pin (num 3) (name 3) (type input))
        (pin (num 4) (name 4) (type input))
        (pin (num 5) (name 5) (type input))
        (pin (num 6) (name 6) (type input))
        (pin (num 7) (name 7) (type input))
        (pin (num 8) (name 8) (type input))
        (pin (num 9) (name 9) (type input))
        (pin (num 10) (name 0) (type input))
        (pin (num 11) (name A) (type input))))
    (libpart (lib Custom_Parts) (part PCA9685)
      (fields
        (field (name Reference) U)
        (field (name Value) PCA9685))
      (pins
        (pin (num 1) (name ADDR_3) (type input))
        (pin (num 2) (name ADDR_4) (type input))
        (pin (num 3) (name LED_0) (type 3state))
        (pin (num 4) (name LED_1) (type 3state))
        (pin (num 5) (name LED_2) (type 3state))
        (pin (num 6) (name LED_3) (type 3state))
        (pin (num 7) (name LED_4) (type 3state))
        (pin (num 8) (name LED_5) (type 3state))
        (pin (num 9) (name LED_6) (type 3state))
        (pin (num 10) (name LED_7) (type 3state))
        (pin (num 11) (name V_SS) (type input))
        (pin (num 12) (name LED_8) (type 3state))
        (pin (num 13) (name LED_9) (type 3state))
        (pin (num 14) (name LED_10) (type 3state))
        (pin (num 15) (name LED_11) (type 3state))
        (pin (num 16) (name LED_12) (type 3state))
        (pin (num 17) (name LED_13) (type 3state))
        (pin (num 18) (name LED_14) (type 3state))
        (pin (num 19) (name LED_15) (type 3state))
        (pin (num 20) (name OE) (type input))
        (pin (num 21) (name ADDR_5) (type input))
        (pin (num 22) (name EXT_CLK) (type input))
        (pin (num 23) (name SCL) (type input))
        (pin (num 24) (name SDA) (type input))
        (pin (num 25) (name V_DD) (type input))
        (pin (num 26) (name ADDR_0) (type input))
        (pin (num 27) (name ADDR_1) (type input))
        (pin (num 28) (name ADDR_2) (type input))
        (pin (num 29) (name PAD) (type input))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Q_NPN_BEC)
      (description "Transistor NPN (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NPN_BEC))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Custom_Parts)
      (uri C:/Users/Kevin/Documents/Projects/KiCadLib/EESCHEMA/Custom_Parts.lib))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib")))
  (nets
    (net (code 1) (name /T3_C_1)
      (node (ref Q22) (pin 3))
      (node (ref T3) (pin 2)))
    (net (code 2) (name /T4_C_2)
      (node (ref T4) (pin 3))
      (node (ref Q33) (pin 3)))
    (net (code 3) (name /T4_C_3)
      (node (ref T4) (pin 4))
      (node (ref Q34) (pin 3)))
    (net (code 4) (name /T4_C_4)
      (node (ref Q35) (pin 3))
      (node (ref T4) (pin 5)))
    (net (code 5) (name /T4_C_5)
      (node (ref T4) (pin 6))
      (node (ref Q36) (pin 3)))
    (net (code 6) (name /T4_C_6)
      (node (ref Q37) (pin 3))
      (node (ref T4) (pin 7)))
    (net (code 7) (name /T4_C_7)
      (node (ref Q38) (pin 3))
      (node (ref T4) (pin 8)))
    (net (code 8) (name /T4_C_8)
      (node (ref Q39) (pin 3))
      (node (ref T4) (pin 9)))
    (net (code 9) (name /T4_C_9)
      (node (ref T4) (pin 10))
      (node (ref Q40) (pin 3)))
    (net (code 10) (name /T3_C_0)
      (node (ref Q21) (pin 3))
      (node (ref T3) (pin 1)))
    (net (code 11) (name /T4_C_1)
      (node (ref Q32) (pin 3))
      (node (ref T4) (pin 2)))
    (net (code 12) (name /T3_C_2)
      (node (ref Q23) (pin 3))
      (node (ref T3) (pin 3)))
    (net (code 13) (name /T3_C_3)
      (node (ref Q24) (pin 3))
      (node (ref T3) (pin 4)))
    (net (code 14) (name /T3_C_4)
      (node (ref Q25) (pin 3))
      (node (ref T3) (pin 5)))
    (net (code 15) (name /T3_C_5)
      (node (ref Q26) (pin 3))
      (node (ref T3) (pin 6)))
    (net (code 16) (name /T3_C_6)
      (node (ref Q27) (pin 3))
      (node (ref T3) (pin 7)))
    (net (code 17) (name /T3_C_7)
      (node (ref T3) (pin 8))
      (node (ref Q28) (pin 3)))
    (net (code 18) (name /T3_C_8)
      (node (ref Q29) (pin 3))
      (node (ref T3) (pin 9)))
    (net (code 19) (name /T3_C_9)
      (node (ref T3) (pin 10))
      (node (ref Q30) (pin 3)))
    (net (code 20) (name /T2_C_0)
      (node (ref Q11) (pin 3))
      (node (ref T2) (pin 1)))
    (net (code 21) (name /T1_C_8)
      (node (ref T1) (pin 9))
      (node (ref Q9) (pin 3)))
    (net (code 22) (name /T1_C_9)
      (node (ref Q10) (pin 3))
      (node (ref T1) (pin 10)))
    (net (code 23) (name /T4_C_0)
      (node (ref T4) (pin 1))
      (node (ref Q31) (pin 3)))
    (net (code 24) (name /T1_C_4)
      (node (ref Q5) (pin 3))
      (node (ref T1) (pin 5)))
    (net (code 25) (name /T1_C_5)
      (node (ref T1) (pin 6))
      (node (ref Q6) (pin 3)))
    (net (code 26) (name /T1_C_6)
      (node (ref T1) (pin 7))
      (node (ref Q7) (pin 3)))
    (net (code 27) (name /T1_C_7)
      (node (ref T1) (pin 8))
      (node (ref Q8) (pin 3)))
    (net (code 28) (name /T1_C_3)
      (node (ref Q4) (pin 3))
      (node (ref T1) (pin 4)))
    (net (code 29) (name /T2_C_9)
      (node (ref T2) (pin 10))
      (node (ref Q20) (pin 3)))
    (net (code 30) (name /T2_C_1)
      (node (ref Q12) (pin 3))
      (node (ref T2) (pin 2)))
    (net (code 31) (name /T2_C_2)
      (node (ref Q13) (pin 3))
      (node (ref T2) (pin 3)))
    (net (code 32) (name /T2_C_3)
      (node (ref T2) (pin 4))
      (node (ref Q14) (pin 3)))
    (net (code 33) (name /T2_C_4)
      (node (ref Q15) (pin 3))
      (node (ref T2) (pin 5)))
    (net (code 34) (name /T2_C_5)
      (node (ref T2) (pin 6))
      (node (ref Q16) (pin 3)))
    (net (code 35) (name /T2_C_6)
      (node (ref Q17) (pin 3))
      (node (ref T2) (pin 7)))
    (net (code 36) (name /T2_C_7)
      (node (ref Q18) (pin 3))
      (node (ref T2) (pin 8)))
    (net (code 37) (name /T2_C_8)
      (node (ref Q19) (pin 3))
      (node (ref T2) (pin 9)))
    (net (code 38) (name /T1_C_0)
      (node (ref Q1) (pin 3))
      (node (ref T1) (pin 1)))
    (net (code 39) (name /T1_C_1)
      (node (ref T1) (pin 2))
      (node (ref Q2) (pin 3)))
    (net (code 40) (name /T1_C_2)
      (node (ref T1) (pin 3))
      (node (ref Q3) (pin 3)))
    (net (code 41) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 42) (name "Net-(Q41-Pad2)")
      (node (ref Q41) (pin 2))
      (node (ref R41) (pin 1)))
    (net (code 43) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 44) (name "Net-(Q41-Pad1)")
      (node (ref U2) (pin 19))
      (node (ref Q41) (pin 1)))
    (net (code 45) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 46) (name "Net-(U2-Pad12)")
      (node (ref U2) (pin 12)))
    (net (code 47) (name "Net-(U2-Pad10)")
      (node (ref U2) (pin 10)))
    (net (code 48) (name "Net-(U2-Pad9)")
      (node (ref U2) (pin 9)))
    (net (code 49) (name "Net-(U2-Pad8)")
      (node (ref U2) (pin 8)))
    (net (code 50) (name "Net-(Q41-Pad3)")
      (node (ref T5) (pin 2))
      (node (ref Q41) (pin 3)))
    (net (code 51) (name /SDA)
      (node (ref U2) (pin 24))
      (node (ref J1) (pin 6))
      (node (ref U1) (pin 24))
      (node (ref U3) (pin 24)))
    (net (code 52) (name /ANODE)
      (node (ref T1) (pin 11))
      (node (ref T3) (pin 11))
      (node (ref T2) (pin 11))
      (node (ref T5) (pin 1))
      (node (ref J2) (pin 5))
      (node (ref J2) (pin 3))
      (node (ref J2) (pin 1))
      (node (ref T4) (pin 11)))
    (net (code 53) (name /nOE)
      (node (ref J1) (pin 5))
      (node (ref U2) (pin 20))
      (node (ref U3) (pin 20))
      (node (ref U1) (pin 20)))
    (net (code 54) (name /SCL)
      (node (ref J1) (pin 4))
      (node (ref U2) (pin 23))
      (node (ref U3) (pin 23))
      (node (ref U1) (pin 23)))
    (net (code 55) (name /GND)
      (node (ref R12) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R15) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 11))
      (node (ref U1) (pin 21))
      (node (ref U1) (pin 2))
      (node (ref U2) (pin 21))
      (node (ref R13) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref U2) (pin 11))
      (node (ref R17) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R33) (pin 2))
      (node (ref U2) (pin 28))
      (node (ref R28) (pin 2))
      (node (ref R29) (pin 2))
      (node (ref R30) (pin 2))
      (node (ref U2) (pin 29))
      (node (ref U3) (pin 28))
      (node (ref R3) (pin 2))
      (node (ref U2) (pin 22))
      (node (ref R27) (pin 2))
      (node (ref U3) (pin 11))
      (node (ref U2) (pin 2))
      (node (ref U3) (pin 1))
      (node (ref U2) (pin 26))
      (node (ref R22) (pin 2))
      (node (ref R32) (pin 2))
      (node (ref R34) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R36) (pin 2))
      (node (ref R37) (pin 2))
      (node (ref R38) (pin 2))
      (node (ref R39) (pin 2))
      (node (ref R35) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref R24) (pin 2))
      (node (ref U3) (pin 21))
      (node (ref U3) (pin 22))
      (node (ref U3) (pin 29))
      (node (ref R25) (pin 2))
      (node (ref R26) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref R41) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref R40) (pin 2))
      (node (ref U1) (pin 22))
      (node (ref J2) (pin 6))
      (node (ref J2) (pin 4))
      (node (ref J2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 29))
      (node (ref U1) (pin 28))
      (node (ref U1) (pin 27))
      (node (ref J1) (pin 3))
      (node (ref J1) (pin 2))
      (node (ref U1) (pin 1)))
    (net (code 56) (name /VDD)
      (node (ref C1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref U2) (pin 25))
      (node (ref U1) (pin 25))
      (node (ref U2) (pin 27))
      (node (ref U1) (pin 26))
      (node (ref U3) (pin 26))
      (node (ref U3) (pin 27))
      (node (ref J1) (pin 1))
      (node (ref U3) (pin 25)))
    (net (code 57) (name /T4_E_7)
      (node (ref R38) (pin 1))
      (node (ref Q38) (pin 2)))
    (net (code 58) (name /T4_E_9)
      (node (ref R40) (pin 1))
      (node (ref Q40) (pin 2)))
    (net (code 59) (name /T4_E_8)
      (node (ref R39) (pin 1))
      (node (ref Q39) (pin 2)))
    (net (code 60) (name /T4_E_6)
      (node (ref R37) (pin 1))
      (node (ref Q37) (pin 2)))
    (net (code 61) (name /T4_E_5)
      (node (ref Q36) (pin 2))
      (node (ref R36) (pin 1)))
    (net (code 62) (name /T4_E_4)
      (node (ref R35) (pin 1))
      (node (ref Q35) (pin 2)))
    (net (code 63) (name /T4_E_3)
      (node (ref R34) (pin 1))
      (node (ref Q34) (pin 2)))
    (net (code 64) (name /T4_E_2)
      (node (ref Q33) (pin 2))
      (node (ref R33) (pin 1)))
    (net (code 65) (name /T4_E_1)
      (node (ref R32) (pin 1))
      (node (ref Q32) (pin 2)))
    (net (code 66) (name /T4_E_0)
      (node (ref Q31) (pin 2))
      (node (ref R31) (pin 1)))
    (net (code 67) (name /T3_G_7)
      (node (ref Q28) (pin 1))
      (node (ref U2) (pin 15)))
    (net (code 68) (name /T4_G_6)
      (node (ref U3) (pin 4))
      (node (ref Q37) (pin 1)))
    (net (code 69) (name /T4_G_5)
      (node (ref Q36) (pin 1))
      (node (ref U3) (pin 7)))
    (net (code 70) (name /T4_G_4)
      (node (ref Q35) (pin 1))
      (node (ref U3) (pin 19)))
    (net (code 71) (name /T4_G_3)
      (node (ref U3) (pin 18))
      (node (ref Q34) (pin 1)))
    (net (code 72) (name /T4_G_2)
      (node (ref Q33) (pin 1))
      (node (ref U3) (pin 5)))
    (net (code 73) (name /T4_G_1)
      (node (ref Q32) (pin 1))
      (node (ref U3) (pin 10)))
    (net (code 74) (name /T4_G_0)
      (node (ref Q31) (pin 1))
      (node (ref U3) (pin 9)))
    (net (code 75) (name /T3_G_9)
      (node (ref Q30) (pin 1))
      (node (ref U3) (pin 12)))
    (net (code 76) (name /T3_G_8)
      (node (ref Q29) (pin 1))
      (node (ref U3) (pin 17)))
    (net (code 77) (name /T4_G_7)
      (node (ref U3) (pin 3))
      (node (ref Q38) (pin 1)))
    (net (code 78) (name /T3_G_6)
      (node (ref U2) (pin 18))
      (node (ref Q27) (pin 1)))
    (net (code 79) (name /T3_G_5)
      (node (ref U3) (pin 15))
      (node (ref Q26) (pin 1)))
    (net (code 80) (name /T3_G_4)
      (node (ref Q25) (pin 1))
      (node (ref U2) (pin 17)))
    (net (code 81) (name /T3_G_3)
      (node (ref Q24) (pin 1))
      (node (ref U2) (pin 16)))
    (net (code 82) (name /T3_G_2)
      (node (ref Q23) (pin 1))
      (node (ref U3) (pin 16)))
    (net (code 83) (name /T3_G_1)
      (node (ref Q22) (pin 1))
      (node (ref U3) (pin 14)))
    (net (code 84) (name /T3_G_0)
      (node (ref U3) (pin 13))
      (node (ref Q21) (pin 1)))
    (net (code 85) (name /T2_G_9)
      (node (ref Q20) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 86) (name /T1_G_6)
      (node (ref U1) (pin 3))
      (node (ref Q7) (pin 1)))
    (net (code 87) (name /T2_G_4)
      (node (ref U2) (pin 4))
      (node (ref Q15) (pin 1)))
    (net (code 88) (name /T2_G_3)
      (node (ref Q14) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 89) (name /T2_G_2)
      (node (ref Q13) (pin 1))
      (node (ref U1) (pin 5)))
    (net (code 90) (name /T2_G_1)
      (node (ref Q12) (pin 1))
      (node (ref U1) (pin 10)))
    (net (code 91) (name /T2_G_0)
      (node (ref U1) (pin 9))
      (node (ref Q11) (pin 1)))
    (net (code 92) (name /T1_G_9)
      (node (ref U1) (pin 12))
      (node (ref Q10) (pin 1)))
    (net (code 93) (name /T1_G_8)
      (node (ref Q9) (pin 1))
      (node (ref U1) (pin 17)))
    (net (code 94) (name /T1_G_7)
      (node (ref U1) (pin 4))
      (node (ref Q8) (pin 1)))
    (net (code 95) (name /T2_G_8)
      (node (ref U1) (pin 6))
      (node (ref Q19) (pin 1)))
    (net (code 96) (name /T1_G_5)
      (node (ref U1) (pin 15))
      (node (ref Q6) (pin 1)))
    (net (code 97) (name /T1_G_4)
      (node (ref U1) (pin 18))
      (node (ref Q5) (pin 1)))
    (net (code 98) (name /T1_G_3)
      (node (ref U1) (pin 19))
      (node (ref Q4) (pin 1)))
    (net (code 99) (name /T1_G_2)
      (node (ref U1) (pin 16))
      (node (ref Q3) (pin 1)))
    (net (code 100) (name /T1_G_1)
      (node (ref U1) (pin 14))
      (node (ref Q2) (pin 1)))
    (net (code 101) (name /T1_G_0)
      (node (ref Q1) (pin 1))
      (node (ref U1) (pin 13)))
    (net (code 102) (name /T4_G_9)
      (node (ref Q40) (pin 1))
      (node (ref U3) (pin 8)))
    (net (code 103) (name /T4_G_8)
      (node (ref Q39) (pin 1))
      (node (ref U3) (pin 6)))
    (net (code 104) (name /T2_G_7)
      (node (ref U2) (pin 6))
      (node (ref Q18) (pin 1)))
    (net (code 105) (name /T2_G_6)
      (node (ref Q17) (pin 1))
      (node (ref U2) (pin 5)))
    (net (code 106) (name /T2_G_5)
      (node (ref U1) (pin 7))
      (node (ref Q16) (pin 1)))
    (net (code 107) (name /T1_E_6)
      (node (ref R7) (pin 1))
      (node (ref Q7) (pin 2)))
    (net (code 108) (name /T2_E_7)
      (node (ref Q18) (pin 2))
      (node (ref R18) (pin 1)))
    (net (code 109) (name /T2_E_8)
      (node (ref Q19) (pin 2))
      (node (ref R19) (pin 1)))
    (net (code 110) (name /T2_E_9)
      (node (ref Q20) (pin 2))
      (node (ref R20) (pin 1)))
    (net (code 111) (name /T1_E_0)
      (node (ref Q1) (pin 2))
      (node (ref R1) (pin 1)))
    (net (code 112) (name /T1_E_1)
      (node (ref Q2) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 113) (name /T1_E_2)
      (node (ref Q3) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 114) (name /T1_E_3)
      (node (ref Q4) (pin 2))
      (node (ref R4) (pin 1)))
    (net (code 115) (name /T1_E_4)
      (node (ref Q5) (pin 2))
      (node (ref R5) (pin 1)))
    (net (code 116) (name /T1_E_5)
      (node (ref Q6) (pin 2))
      (node (ref R6) (pin 1)))
    (net (code 117) (name /T2_E_6)
      (node (ref R17) (pin 1))
      (node (ref Q17) (pin 2)))
    (net (code 118) (name /T1_E_7)
      (node (ref R8) (pin 1))
      (node (ref Q8) (pin 2)))
    (net (code 119) (name /T1_E_8)
      (node (ref Q9) (pin 2))
      (node (ref R9) (pin 1)))
    (net (code 120) (name /T1_E_9)
      (node (ref Q10) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 121) (name /T3_E_7)
      (node (ref Q28) (pin 2))
      (node (ref R28) (pin 1)))
    (net (code 122) (name /T3_E_0)
      (node (ref Q21) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 123) (name /T3_E_1)
      (node (ref Q22) (pin 2))
      (node (ref R22) (pin 1)))
    (net (code 124) (name /T3_E_2)
      (node (ref Q23) (pin 2))
      (node (ref R23) (pin 1)))
    (net (code 125) (name /T3_E_3)
      (node (ref Q24) (pin 2))
      (node (ref R24) (pin 1)))
    (net (code 126) (name /T3_E_4)
      (node (ref R25) (pin 1))
      (node (ref Q25) (pin 2)))
    (net (code 127) (name /T3_E_5)
      (node (ref R26) (pin 1))
      (node (ref Q26) (pin 2)))
    (net (code 128) (name /T3_E_6)
      (node (ref Q27) (pin 2))
      (node (ref R27) (pin 1)))
    (net (code 129) (name /T3_E_8)
      (node (ref R29) (pin 1))
      (node (ref Q29) (pin 2)))
    (net (code 130) (name /T3_E_9)
      (node (ref Q30) (pin 2))
      (node (ref R30) (pin 1)))
    (net (code 131) (name /T2_E_0)
      (node (ref R11) (pin 1))
      (node (ref Q11) (pin 2)))
    (net (code 132) (name /T2_E_1)
      (node (ref R12) (pin 1))
      (node (ref Q12) (pin 2)))
    (net (code 133) (name /T2_E_2)
      (node (ref R13) (pin 1))
      (node (ref Q13) (pin 2)))
    (net (code 134) (name /T2_E_3)
      (node (ref R14) (pin 1))
      (node (ref Q14) (pin 2)))
    (net (code 135) (name /T2_E_4)
      (node (ref Q15) (pin 2))
      (node (ref R15) (pin 1)))
    (net (code 136) (name /T2_E_5)
      (node (ref Q16) (pin 2))
      (node (ref R16) (pin 1)))))