(export (version D)
  (design
    (source C:/Users/Kevin/Documents/Projects/NixieTubeClock/Nixie_IN8_Breakout/Nixie_IN8_Breakout.sch)
    (date "5/26/2017 8:02:41 PM")
    (tool "Eeschema 4.0.6")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Nixie_IN8_Breakout.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref T1)
      (value IN-8)
      (footprint "Custom Parts:IN-8")
      (libsource (lib Custom_Parts) (part IN-8))
      (sheetpath (names /) (tstamps /))
      (tstamp 590F8FF1))
    (comp (ref J1)
      (value CONN_02X06)
      (footprint Pin_Headers:Pin_Header_Angled_2x06_Pitch2.54mm)
      (libsource (lib conn) (part CONN_02X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 591006B6)))
  (libparts
    (libpart (lib conn) (part CONN_02X06)
      (description "Connector, double row, 02x06, pin header")
      (footprints
        (fp Pin_Header_Straight_2X*)
        (fp Pin_Header_Angled_2X*)
        (fp Socket_Strip_Straight_2X*)
        (fp Socket_Strip_Angled_2X*)
        (fp IDC_Header_Straight_*))
      (fields
        (field (name Reference) J)
        (field (name Value) CONN_02X06))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))
        (pin (num 5) (name P5) (type passive))
        (pin (num 6) (name P6) (type passive))
        (pin (num 7) (name P7) (type passive))
        (pin (num 8) (name P8) (type passive))
        (pin (num 9) (name P9) (type passive))
        (pin (num 10) (name P10) (type passive))
        (pin (num 11) (name P11) (type passive))
        (pin (num 12) (name P12) (type passive))))
    (libpart (lib Custom_Parts) (part IN-8)
      (fields
        (field (name Reference) T)
        (field (name Value) IN-8))
      (pins
        (pin (num 1) (name 1) (type input))
        (pin (num 2) (name 2) (type input))
        (pin (num 3) (name 3) (type input))
        (pin (num 4) (name 4) (type input))
        (pin (num 5) (name 5) (type input))
        (pin (num 6) (name 6) (type input))
        (pin (num 7) (name 7) (type input))
        (pin (num 8) (name 8) (type input))
        (pin (num 9) (name 9) (type input))
        (pin (num 10) (name 0) (type input))
        (pin (num 11) (name Anode) (type input)))))
  (libraries
    (library (logical Custom_Parts)
      (uri C:\Users\Kevin\Documents\Projects\KiCadLib\EESCHEMA\Custom_Parts.lib))
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib")))
  (nets
    (net (code 1) (name /2)
      (node (ref J1) (pin 6))
      (node (ref T1) (pin 2)))
    (net (code 2) (name /3)
      (node (ref J1) (pin 8))
      (node (ref T1) (pin 3)))
    (net (code 3) (name /4)
      (node (ref T1) (pin 4))
      (node (ref J1) (pin 10)))
    (net (code 4) (name /5)
      (node (ref T1) (pin 5))
      (node (ref J1) (pin 12)))
    (net (code 5) (name /6)
      (node (ref T1) (pin 6))
      (node (ref J1) (pin 11)))
    (net (code 6) (name /7)
      (node (ref J1) (pin 9))
      (node (ref T1) (pin 7)))
    (net (code 7) (name /8)
      (node (ref J1) (pin 7))
      (node (ref T1) (pin 8)))
    (net (code 8) (name /9)
      (node (ref T1) (pin 9))
      (node (ref J1) (pin 5)))
    (net (code 9) (name /0)
      (node (ref T1) (pin 10))
      (node (ref J1) (pin 3)))
    (net (code 10) (name /A)
      (node (ref J1) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref T1) (pin 11)))
    (net (code 11) (name /1)
      (node (ref J1) (pin 4))
      (node (ref T1) (pin 1)))))